This folder holds the needed and optional pcb gerber files for the 1250XL project.
They are:
1250XLv1_4 -- Mainboard
Cartridge Pin Holder  -  a simple pcb to align the pins of the original Atari 1200XL cartridge connector with the mainboard for soldering.  PCB thickness should not exceed 1mm when ordering from the board house.
PBI Riser – This is a work around for the 1200XL case design that is not deep enough to handle a PBI connector.
StereoAudioOut – optional for PokeyMax 2B/4 stereo audio output, mounted on mainboard using two screws, nuts and spacer in the old RF output on the 1200XL case.
Sophia2MiniHDMI – optional for Sophia video upgrade, uses same connecting cable in Sophia kit using two screws, nuts and spacer in the old channel switch position on the 1200XL case.

